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Enabling Independence through Technology
Door Operator Information – Label Next 120
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Your new door operator will look like the image above.

To ensure the maximum reliability from your system we recommended it should be serviced every 12 months.

If a maintenance agreement is already in place with us we will automatically contact you to arrange a convenient date & time for a service visit.  

Opening the Door
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The door operator will normally have been installed with a key fob and/or push button (see sample images above). 

To operate the door press the button provided and the door will operate for the time requested at installation (typically 8-15 seconds), or alternatively the system can be set so that the button opens the door on first press and closes on a further press.
You can also open the door manually if required by either pushing or pulling the door open. However, it is important that the door is not forced to close as this will damage the operator. Let the door close automatically.

It is important that the door is NOT manually locked with the key.   If this is required, the operator should be switched into manual or off. Operation of the opener whilst the door is locked will damage the unit.

Door operator mode selector
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AI-generated content may be incorrect.]The mode selector has multiple options.
To change the current mode, press the ‘SET’ button (middle button @ bottom), every time you press the ‘SET’ button it will cycle to the next option/mode (the display will show current mode that is selected), Once you have found the required option wait 5 seconds and that mode will be selected for you.


· For normal operation of the door from the key fobs etc the key should be in ‘2 WAY’.

· For the door to be in the open permanently the option should be in ‘DOOR OPEN’.

· For the door to be used manually only, the option should be in ‘MANUAL’.

Safety Sensors
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These are fitted to both sides of the door. These sensors stop the door from operating if anyone or anything is positioned in front or behind the door when it is moving. It is important that they are kept clean and not covered up otherwise the operator will no longer work, which will stop the operator from working.

Trouble shooting
If you are having any difficulty in operating the door:
1. Ensure the operator is switched ‘On’ and set to ‘2 Way’
2. Check that there is no objects which may be interfering with the range of the safety sensors or physically blocking the movement of the door 
Examples:  Something behind the door, door catching on the on the floor, dirty sensors, post not pushed fully through the letter box.
3. Switch the door operator ‘Off’, leave for 1 minute, and then switch it back ‘ON’.
4. Ensure that the batteries in the key fob or wall buttons are functioning & do not require replacing

If problems persist, please contact us using the details at the end of these instructions

Should you experience any issues or have any questions please contact us:

DH2 Solutions Ltd
Unit 25G2, Springfield Commercial Centre, Bagley Lane, Leeds, LS28 5LY
Telephone: 0113 2564572
Web: DH2Solutions.co.uk
Email: info@dh2solutions.co.uk
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